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PART 1 GENERAL
1.1 SUMMARY
A. Section includes:
1. Sound-absorptive, micro-perforated acoustic panels finished in real wood veneer. SoundPly’s ® fully enclosed system is lightweight and performs efficiently with no backloading required.
B. Related sections
1. Section 01350 – Special Environmental Requirements
2. Section 09800 – Acoustical Treatment
3. Section 092116 – Gypsum Board Assemblies (by others)
1.2 REFERENCES
A.    Test Methods:
1. ASTM C423 Sound absorption and sound absorption coefficients by the reverberation room method performed by an independent testing agency.
2. ASTM E84 Standard test method for surface burning characteristics of building materials.
3. ASTM D1037 Linear expansion with change in moisture content.
 
4.    Standard Method Version 1.2 for CDPH01350 Volatile organic compounds.
1.3 QUALITY ASSURANCE
A. Single Source Responsibility: Provide acoustic panels from a single manufacturer with at least 5 years of prior experience fabricating projects of similar size and complexity.
B. Installer Qualifications: Installation shall be done by qualified carpenters with at least 2 years’ experience in the installation of architectural woodwork or acoustical wall material. Installers must receive training on handling, cutting, machining, and field finishing the specified product prior to receiving materials on site.
C. Fire Performance Characteristics: Class A as tested by an independent accredited testing facility. Tests: ASTM E84. Flame spread: 25 or less. Smoke developed: 450 or less as specified by state or local codes.
D. Applicable LEED Credits: 

LEED v4/v4.1(Deadline End of June 2027):

1. MRc4 Recycled Content
2. EQ 4.4 Low-Emitting Materials
3. Material Ingredient Disclosure-Option 1
4. EQ 9 Enhanced Acoustical Performance
LEED v5(launched April 2025):
1. MRc4 Recycled Content (Building Product Selection and Procurement)
2. Material Ingredients Disclosure-Option 1(Building Product Disclosure and Optimization)
3. Low-Emitting Materials (Materials and Resources)
4. Sound Environment (Indoor Environmental Quality (EQ)-Occupant Experience)
E. Coordination of Work: Installing contractor shall organize and conduct a pre-installation survey of temperature, humidity, and construction elements attaching, penetrating, or concealed behind the acoustic wall panels.
1.4 SUBMITTALS
1. Comply with Section 013300 – Submittal Procedures
1. Product Data: Manufacturer’s technical data and installation instructions for each type of wall panel required. 
1. Certifications: Certified test reports showing compliance with performance requirements specified.
1. Samples: Submit samples of each panel type and finish type required. Include samples that show the range of variation expected in grain, texture and color. 
1. Shop Drawings: Submit shop drawings, including details, for all ceilings. Coordinate wall panel layout, installation and suspension system components. Show overall layout with dimensions and details of penetrations and intersections with other materials or building components.
1. LEED Requirements: Where specified, submit required documentation indicating compliance.
1. Submit operation and maintenance data for installed products. Include precautions relating to harmful cleaning materials and methods that would affect the service life of the panels.
1.5	DELIVERY, STORAGE AND HANDLING
A. Deliver panels to the project in original, unopened packages. Inspect containers for visible damage and report any questionable condition to the shipper and manufacturer immediately.
B. Store products in a fully enclosed, clean, dry space out of direct sunlight and protected from damage with temperature controlled between 50 and 86 degrees F.
C. Before installing, product must acclimate in intended installation area and must be done at the intended operational temperature and humidity. This procedure of acclimatization is a length of at least 72 hours.
D. Handle products carefully to avoid damaging panel surfaces or chipping edges. Report any damage immediately. Installation of damaged panels is not covered by the manufacturer’s warranty.
1.6 PROJECT CONDITIONS
A. Do not install acoustic panels until space is enclosed and weather-proofed, wet work is completely dry and ambient temperature and humidity conditions are maintained at the levels indicated for the project when occupied for its intended use.
B. Permit panels to reach room temperature, 50 to 86 degrees F, and stabilized moisture content of 25% to 55% RH for at least 72 hours before installation per AWI standards. Building should be enclosed and HVAC systems functioning in continuous operation with relative humidity maintained between 25 and 55 percent.
1.7 WARRANTY
A. Provide manufacturer’s standard one-year written product warranty per Section 01770 – Closeout Procedures
B. Manufacturer’s warranty is limited to decorative or acoustical panel materials only. Other components used in the set up are excluded. Refer to the appropriate provisions in the related specification section.  
1.8 MAINTENANCE
A. Maintenance Instructions: Provide manufacturer’s standard maintenance and cleaning instructions for finishes provided.
PART 2 – PRODUCTS
2.1 MANUFACTURER
A. Provide SoundPly® panels manufactured by Navy Island Inc., 275 Marie Avenue E, St. Paul, MN 55118, Ph. (651) 451-4454, email soundply@navyisland.com
2.2 MATERIALS
A. SOUNDPLY® Latus RFM Panels for Interior Installation: Select 
Latus RF-M19 (3/4”) or Latus RF-M25 (1”) or Latus RF-M38 (1 ½”) or Latus RF-M51 (2”) thick acoustical panels as follows: Real wood veneer laminated to a fiberglass reinforced polymer or a painted surface applied to an MDF skin. Surface skin thickness shall not be less than 1.5mm (0.060”). The core of the panels shall be comprised of a Class A sintered resin-reinforced glass wool. 
B. Panel Edge Treatment: Panels will be edge banded with the matching materials and finish, or as specified by the architect, to match with the panel face. 
C. Reveal Options: Select Panels to be mounted per manufacturer’s installation instructions for open reveal with provided hardware from Navy Island (1/8”, 1/4”)
D. Panel Weight: RF-M19 = 2.2 lbs./ft2, RF-M25 = 1.6 lbs./ft2, RF-M38 = 3.0 lbs./ft2, RF-M51 = 3.3 lbs./ft2. 
E. Panel Sizes: Select Panels are available in custom sizes up to 60” x 120” 
F. Panel Thickness: Select RF-M19 (3/4”), RF-M25 (1”), RF-M38 (1 1/2”), RF-M51 (2”)
G. Flame Resistance: Latus RF Panels have a Class 1(A) rating based on ASTM E84 standard test method for surface burning characteristics in building materials. Depending on the use and the type of veneer selected, Latus Panels can be used in Class A environments (IBC Chapter 8 Section 803)
H. Perforations: Panels will be furnished with perforated faces consisting of 0.5mm (0.02”) diameter holes in an offset pattern. The perforations must be clean without rounded edges or grain pull out between perforations. A minimum of 99.5% of the perforations must be acoustically functional, providing unobstructed passage into the core. Perforations must maintain consistent diameter through the face material and backer with no tapering or roughness. 
I. Acoustic Performance: To generate the standing sound waves required for resistive absorption, each panel must have an acoustically reflective back surface that extends the panel’s full length and width. Each panel must achieve a minimum NRC test value as stated without any cavity space or back loading: Select 

- Latus RF-M19 (3/4” thick) .70 NRC 
- Latus RF-M25 (1” thick) .90 NRC 
- Latus RF-M38 (1 1/2” thick) .95 NRC 
- Latus RF-M51 (2” thick) 1.0 NRC 
J. Panel Stability: Linear contraction or expansion to not exceed 0.4% maximum variation in width or height per ASTM D1037.
K. VOC Emissions: Panels must be third party certified to be in compliance with CDPH01350 for volatile organic compounds.
L. Finish for Veneer Faced Panels: Select 
1. Species as selected by the architect.	
2. Cut: plain sliced, quartered/rift
3. Matching veneer leaves: random match.
4. Finishes shall be applied in the shop: clear or painted.

2.3 ACCESSORIES
A. Hardware supplied by Navy Island and used per manufacturers mounting
PART 3 – EXECUTION
3.1 EXAMINATION
A. Inspect installation area and conditions under which work is to be performed for compliance with all manufacturer’s environmental requirements. All wet work in the installation area must be complete, cured and dry prior to installation. Do not proceed until all unsatisfactory conditions have been corrected.
3.2 PREPARATION
A. Clean surfaces thoroughly before installation.
B. Install should not begin until all substrates, and the ceiling layout are properly prepared to conform with approved shop drawings.
C. Protect all adjacent surfaces from possible damage during installation of material.
D. It is the contractor’s responsibility to provide required support to install suspension system without interference with other elements and perimeters
E. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under project conditions
3.3 INSTALLATION
A. Installation must be done by qualified carpenters with 2 years’ experience in the installation of architectural woodwork or acoustic systems. The firm must demonstrate successful experience installing materials of similar type and quality of those required for this project. The use of proper carpentry tools and techniques will be required for the installation. 
B. Comply with manufacturer’s instructions and recommendations for hanging panels.
C. Confirm all field dimensions are coordinated with shop drawings.
3.4 ADJUSTING AND CLEANING
A. Clean soiled surfaces of panels per manufacturer’s instructions.
B. Remove and replace damaged or discolored materials not in compliance with manufacturer’s tolerances.
Contact information: 
Navy Island, Inc.
275 Marie Ave. E.
West St. Paul, MN 55118
651-451-4454
soundply@navyisland.com
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