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PART 1 GENERAL
1.1 SUMMARY
A. Section includes:
Sound-absorptive, micro-perforated acoustic planks finished in real wood veneer. SoundPly’s ® fully enclosed system is lightweight and performs efficiently with no backloading required.
B. Related sections:
1. Section 01350 – Special Environmental Requirements
Section 092116 – Gypsum Board Assemblies (by others)
Section 09800 – Acoustical Treatment
Section 095300- Acoustical Ceiling Suspension Systems (by others) 
Section 095100- Acoustical Ceilings 
1.2 REFERENCES
A. Test Methods:
1. ASTM C423 Sound absorption and sound absorption coefficients by the reverberation room method performed by an independent testing agency.
2. ASTM E84 Standard test method for surface burning characteristics of building materials.
3. ASTM D1037 Linear expansion with change in moisture content.
1.3 QUALITY ASSURANCE
A. Single Source Responsibility: Provide acoustic planks from a single manufacturer with at least 5 years of prior experience fabricating projects of similar size and complexity.
B. Installer Qualifications: Installation shall be done by qualified carpenters with at least 2 years’ experience in the installation of architectural woodwork or acoustical systems. Installers must receive training on handling, cutting, machining and field finishing the specified product prior to receiving materials on site.
C. Fire Performance Characteristics: Class A as tested by an independent accredited testing facility. Tests: ASTM E84. Flame spread: 25 or less. Smoke developed: 450 or less as specified by state or local codes.
D. Applicable LEED Credits: 
LEED v4/v4.1(Deadline End of June 2027):
1. MRc4 Recycled Content
2. Material Ingredient Disclosure-Option 1
3. EQ 9 Enhanced Acoustical Performance
LEED v5(launched April 2025):
1. MRc4 Recycled Content (Building Product Selection and Procurement)
2. Material Ingredients Disclosure-Option 1(Building Product Disclosure and Optimization)
3. Sound Environment (Indoor Environmental Quality (EQ)-Occupant Experience)
E. Coordination of Work: Installing contractor shall organize and conduct a pre-installation survey of temperature, humidity and construction elements attaching, penetrating, or concealed behind the acoustic planks.
1.4 SUBMITTALS
A. Comply with Section 013300 – Submittal Procedures

B. Product Data: Manufacturer’s technical data and installation instructions for each type of plank required. 
C. Certifications: Certified test reports showing compliance with performance requirements specified.
D. Samples: Submit samples of each panel type and finish type required. Include samples that show the range of variation expected in grain, texture and color. 
E. Shop Drawings: Submit shop drawings, including details, for all surfaces. Coordinate plank layout, installation, and suspension system components. Show overall layout with dimensions and details of penetrations and intersections with other materials or building components.
F. LEED Requirements: Where specified, submit required documentation indicating compliance.
G. Submit operation and maintenance data for installed products. Include precautions relating to harmful cleaning materials and methods that would affect the service life of the planks.
1.5 DELIVERY, STORAGE AND HANDLING
A. Deliver planks to the project in original, unopened packages. Inspect containers for visible damage and report any questionable condition to the shipper and manufacturer immediately.
B. Store products in a fully enclosed, clean, dry space out of direct sunlight and protected from damage with temperature controlled between 50 and 86 degrees F.
C. Before installing, product must acclimate in intended installation area and must be done at the intended operational temperature and humidity. This procedure of acclimatization is a length of at least 72 hours.
D. Handle products carefully to avoid damaging plank surfaces or chipping edges. Report any damage immediately. Installation of damaged planks is not covered by the manufacturer’s warranty.
1.6 PROJECT CONDITIONS
0. Do not install acoustic planks until space is enclosed and weather-proofed, wet work is completely dry and ambient temperature and humidity conditions are maintained at the levels indicated for the project when occupied for its intended use.
1. Permit planks to reach room temperature, 50 to 86 degrees F, and stabilized moisture content of 25% to 55% RH for at least 72 hours before installation per AWI standards. Building should be enclosed and HVAC systems functioning in continuous operation with relative humidity maintained between 25 and 55 percent.
1.7 WARRANTY
A. Provide manufacturer’s standard one-year written product warranty per Section 01770 – Closeout Procedures
B. Manufacturer’s warranty is limited to decorative or acoustical plank materials only. Other components used in the acoustic system are excluded. Refer to the appropriate provisions in the related specification section.  
1.8 MAINTENANCE
A. Maintenance Instructions: Provide manufacturer’s standard maintenance and cleaning instructions for finishes provided.
PART 2 – PRODUCTS
2.1 MANUFACTURER
A. Provide planks utilizing SoundPly® acoustic panels manufactured by Navy Island Inc., 275 Marie Avenue E, St. Paul, MN 55118, Ph. (651) 451-4454, email soundply@navyisland.com
2.2 MATERIALS
A. SOUNDPLY® Lino LRM Planks for Interior Installation: Select 
Lino LR-M19 (3/4”) or Lino LR-M25 (1”) or Lino LR-M38 (1 1/2”) or Lino LR-M51 (2”) thick acoustical planks as follows: Real wood veneer laminated to a fiberglass reinforced polymer or a painted surface applied to an MDF skin. Surface skin thickness shall not be less than 1.5mm (0.060”). The core of the planks shall be comprised of a Class A mineral wool. 
1. Plank Edge Treatment: Planks will be edge banded with the matching materials and finish, or as specified by the architect, to match or contrast with the plank face.
1. Planks Spacing: Select Planks to be mounted per manufacturer’s installation instructions for open reveal (1/8”, 1/4") 
2. Planks Weight: LR-M19 = 2.2 lbs./ft2, LR-M25 = 2.3 lbs./ft2, LRM-38 = 2.8 lbs./ft2, LRM-51 = 3.6 lbs./ft2. 
3. Planks Sizes: Select Planks are available in the following sizes: 
A. Plank Width: nominal 6”, 8”, 12”, (actual 5 7/8”, 7 7/8” or 11 7/8”). 
B. Plank Length:  A mix of 8’ and 10’
4. Plank thickness: Select LR-M19 (3/4”), LR-M25 (1”), LR-M38 (1 1/2”), LR-M51 (2”)
5. Flame Resistance: Lino Planks are composed of SoundPly® LRM panels which have a Class 1(A) rating based on ASTM E84 standard test method for surface burning characteristics in building materials. Depending on the use and the type of veneer selected, Lino Planks can be used in Class A environments (IBC Chapter 8 Section 803).
6. Perforations: Planks will be furnished with perforated faces consisting of 0.5mm (0.02”) diameter holes in an offset pattern. The perforations must be clean without rounded edges or grain pull out between perforations. A minimum of 99.5% of the perforations must be acoustically functional, providing unobstructed passage into the core. Perforations must maintain consistent diameter through the face material and backer with no tapering or roughness. 
7. Acoustic Performance: To generate the standing sound waves required for resistive absorption, each plank must have a solid acoustically reflective back surface that extends the plank’s full length and width. Each plank must achieve a minimum NRC test value as stated without any cavity space or back loading: Select 
- Lino LR-M19 (3/4” thick) .70 NRC 
- Lino LR-M25 (1” thick) .80 NRC 
- Lino LR-M38 (1 1/2” thick) .85 NRC 
- Lino LR-M51 (2” thick) .95 NRC 
8. Plank Stability: Linear contraction or expansion to not exceed 0.4% maximum variation in width or height per ASTM D1037.
9. Finish for Veneer Faced Planks: Select 
a. Species as selected by the architect.	
b. Cut: plain sliced, quartered/rift
c. Finishes shall be applied in the shop: clear or painted.
2.3 ACCESSORIES
A. Hardware supplied by Navy Island and used per manufacturers mounting.
PART 3 – EXECUTION
3.1 EXAMINATION
A. Inspect installation area and conditions under which work is to be performed for compliance with all manufacturer’s environmental requirements. All wet work in the installation area must be complete, cured, and dry prior to installation. Do not proceed until all unsatisfactory conditions have been corrected.
3.2 PREPARATION
A. Clean surfaces thoroughly before installation.
B. Install should not begin until all substrates, and the wall layout are properly prepared to conform with approved shop drawings.
C. Protect all adjacent surfaces from possible damage during installation of material.
D. Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under project conditions.
3.3 INSTALLATION
A. Installation must be done by qualified carpenters with 2 years’ experience in the installation of architectural woodwork or acoustic systems. The firm must demonstrate successful experience installing materials of similar type and quality of those required for this project. The use of proper carpentry tools and techniques will be required for the installation. 
B. Comply with manufacturer’s instructions and recommendations for installing planks.
1. For a suspended grid, install using Plank Clips supplied by Navy Island, which impale securely onto a plank’s edge, then fasten to the 15/16” heavy duty suspended grid. Grid can be provided by one of Navy Island’s recommended suppliers (USG or Chicago Metallic).
2. For direct mount, install using Plank Clips supplied by Navy Island, which are impaled securely onto a plank’s edge and fastened to a pre-installed 15/16” hat channel or pre-installed level furring strips using self-tapping screws. 
C. Confirm all field dimensions are coordinated with shop drawings.
3.4 ADJUSTING AND CLEANING
A. Clean soiled surfaces of planks per manufacturer’s instructions.
B. Remove and replace damaged or discolored materials not in compliance with manufacturer’s tolerances.
Contact information: 
Navy Island, Inc.
275 Marie Ave. E.
West St. Paul, MN 55118
651-451-4454
soundply@navyisland.com
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